;Title of the problem

;-------------------

INFILTRATION IN HOMOGENEOUS COLUMN OF SAND

;-------------------------------------------

; KODE: 1 mixed form FD (MFD); 2: h form FD (HFD); 3: h form FE (HFE);

; 4:teta form FD (TFD)

; 5:teta form FE (TFE)

; KBLOCK: code to choose the way for calculating interblock conductivity:

; 1: arithmetic mean; 2: harmonic mean; 3: geometric mean; 4: upstream

; KBOUN: code for boundary conditions 0: constant h o theta; 1: constant rate

;-------------------------------------------------

;NNODE NMAT NLAY KODE KREST KBOUN KBLOCK

;-------------------------------------------------

60 4 1 1 0 0 1

;------------------------------------------------------------------------------

; IM KS(IM) PA(IM) ALFA(IM) BETA(IM) GAMMA(IM) TETAS(IM) TETAR(IM)

;------------------------------------------------------------------------------

; Sand (type 1)

1 9.44E-3 1.175E+6 1.611E+6 4.74 3.96 0.287 0.075

; Yolo light clay (type 2)

10 1.23E-5 124.6 739. 1.77 4.0 0.495 0.124

; Berino (type 3)

20 6.26E-3 0.0 2.80E-2 2.239 0.553 0.3658 0.0286

; Glendale (type 3)

21 1.516E-4 0.0 1.04E-2 1.3954 0.283 0.4686 0.1060

;

;----------------- Control data-------------------------------

;DTMIN DTPRINT TPRINT ITERMX NSTEPS TINIZ TFINAL EPS

;-------------------------------------------------------------

1.D-5 200. 200. 30 100000 0. 4000. 1.D-8

;---------------------------------------

;ZMIN DZ DT DTMAX DMUL DDIV NLIM

;---------------------------------------

0.0 2. 1.D-6 10.D0 1.1 0.5 10

;-------------

; Initial data

;--------------

; N HO

;--------------

1 -20.0

2 -100.

60 -100.

;---------------

; Material codes

;---------------

; N IMAT(N)

1 1

60 1

; Restart data

;--------------------

; VWI CVWI CVWO

;--------------------

; 0 0. 0.

;-------

; RATE

;-------

2.E-3